

|  |  |
| --- | --- |
| **КАНЦЕРН «БЕЛЛЯСПАПЕРПРАМ»**  **АДКРЫТАЕ АКЦЫЯНЕРНАЕ ТАВАРЫСТВА**  **«РЭЧЫЦАДРЭЎ»**  **ААТ «РЭЧЫЦАДРЭЎ»**  вул. Х лет Кастрычніка, 17/19, 247500 г. Рэчыца  генеральны дырэктар +375(02340) 6-22-70  галоўны бухгалтар (02340) 2 31 17  факс (02340) 2 66 50  б/р 3012096420015 у ф-ле № 323  ОАО «АСБ Беларусбанк» у г. Рэчыца код 661  УПН 400025915 ОКПО 00276417 | **КОНЦЕРН «БЕЛЛЕСБУМПРОМ» ОТКРЫТОЕ АКЦИОНЕРНОЕ ОБЩЕСТВО**  **«РЕЧИЦАДРЕВ»**  **ОАО «РЕЧИЦАДРЕВ»**  ул. Х лет Октября, 17/19, 247500 г. Речица  генеральный директор +375 (02340) 6-22-70  главный бухгалтер (02340) 2 31 17 факс (02340) 2 66 50  р/с 3012096420015 в ф-ле № 323  ОАО «АСБ Беларусбанк» в г. Речица код 661  УПН 400025915 ОКПО 00276417 |

**Commercial offer**

**Dear Sirs,**

The joint stock company “Rechytsadrev” is one of the largest up-to-date woodworking industry enterprises in the Republic of Belarus. We enterprise specializes in preparation and production of plywood, chipboard, laminated chipboard, home and office furniture, fuel briquettes.

We are glad to offer you the delivery of the following production:

****Chipboard (State Standards of the Republic of Belarus 1348-2009)**** Code — 4410111000

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name of production | Grades | Unit of measure | Size of a sheet, mm | Emission class | Base price in euro  for 1 m3 without VAT |
| ****Chipboard**** | 1 | M3 | 2750x1830x15  2750x1830x16 | E-1 | 85 |
| 1 | 85 |

****Laminated chipboard****

****(Technical Regulations of the Republic of Belarus 200100328.002-2001)**** Code— 441011300

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name of production | Unit of measure | Size of a sheet, mm | Emission class | Base price in euro for 1 m2 without VAT |
| ****Laminated chipboard**** | m2 | 2750x1830x16 | E-1 | 2,6 |

The production facilities of the enterprise allow producing laminated chipboard of thickness from 8 to 42 mm.

**Decors:** the production of LLC Schattdekor, Shatura, Russia.

**Stamping type:** (PR) wood pores, shagreen (PE).

Maximum standard loading of transport unit:

Wagon (64t) 1100 sheets – 5535,75 m2

Motor transport (19,080/20,040t) – 1811,7 m2

**Delivery basic terms:** 100% prepayment, FCA, Rechytsa.

**Production sales terms:** direct negotiations.

Phone/fax +375 2340 63325, +375 2340 65418 (chipboard, laminated chipboard)

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Plywood**  **(State Standards of the Republic of Belarus 1348-2009) Code — 4412321000**  Size of a sheet 1525х1525 mm | | | | | | | | |
|  | | | | | | | | |
| Offer price in euro for 1 m3 without VAT | | | | | | | | |
| **Grades** | **1/2 pol** | **2/2 pol** | **2/3 pol** | **2/4 pol** | **3/3 pol** | **3/4 pol** | **4/4 unpol** |  |
| **Thickness** |
| **3** | **535** | **491** | **487** | **451** | **419** | **413** | **364** |  |
| **4** | **410** | **390** | **385** | **368** | **372** | **345** | **330** |  |
| **5** | **416** | **368** | **345** | **338** | **335** | **319** | **311** |  |
| **6** | **413** | **366** | **338** | **330** | **326** | **317** | **302** |  |
| **8** | **399** | **344** | **328** | **307** | **307** | **289** | **280** |  |
| **9** | **398** | **340** | **327** | **305** | **307** | **289** | **273** |  |
| **10** | **398** | **337** | **327** | **306** | **303** | **280** | **270** |  |
| **12** | **372** | **329** | **315** | **293** | **293** | **272** | **255** |  |
| **15** | **372** | **317** | **315** | **293** | **293** | **272** | **255** |  |
| **18** | **372** | **317** | **315** | **293** | **293** | **272** | **255** |  |
| **21** | **397** | **327** | **323** | **293** | **293** | **272** | **255** |  |
|  |  |  |  |  |  |  |  |  |

**We also offer fuel wood briquettes (wood dust), code — 4401399000, at a price 60 Euro for 1t without VAT (in the Summer).**

The size of the briquette: 40-110\*150\*60mm / Lower heating value 16600 kJ/kg  
The density of the granules is not less than 800 kg/m3 / A moisture content not exceeding 12%

The ash content of not more than 0.4% / The sulfur content of not more than 0.15%   
The nitrogen content of not more than 2.5%

Briquettes are Packed in heat-sealed polyethylene bags of 12 pieces.  
Net weight of the briquettes in the bag is about 10 kg.

Phone/fax +375 2340 63050 (plywood, fuel briquettes).

